Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1729	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	25/06/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7958   GPS	Rainfall:	No Data
	Northing/Long.:	7801892 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	305624  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Ferrosol     	Principal Profile Form:	Gn3.12
	ASC Confidence:	Great Soil Group:	Euchrozem
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - None recorded
	Mid Strata - Tree, 1.01-3m, Isolated plants. *Species includes - Eucalyptus crebra
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana, Brachychiton 
	Surface Coarse Fragments:	2-10%, bouldery, 600mm-2m, subangular, Basalt
	Profile Morphology
	A11	0 - 0.05 m	Dark reddish brown (5YR3/4-Moist); ; Clay loam (Heavy); Weak grade of structure, 2-5 mm, Platy; 
	Smooth-ped fabric; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 
	(Raupach, 0.02); Clear change to - 
	B1	0.05 - 0.32 m	Dark reddish brown (2.5YR3/4-Moist); ; Light clay; Massive grade of structure; Weak grade of 
	structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Dry; Very firm consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.5 (Raupach, 0.2); Gradual change to - 
	B21	0.32 - 0.8 m	Dark red (2.5YR3/6-Moist); ; Light medium clay; Strong grade of structure, 5-10 mm, Polyhedral; 
	Smooth-ped fabric; Dry; Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 
	(Raupach, 0.4); Field pH 7 (Raupach, 0.8); 
	B22	0.8 - 0.9 m	; Smooth-ped fabric; Dry; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1729	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1729	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile