Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1743	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	11/05/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8055   GPS	Rainfall:	No Data
	Northing/Long.:	7662732 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	358916  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	8 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Fluvic Bleached-Leptic Tenosol Medium Slightly 	Principal Profile Form:	Uc2.12
	gravelly Sandy Not recorded Shallow
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Hummock grass, 0.51-1m, Mid-dense. *Species includes - Triodia mitchelii, Aristida species, Eriachne 
	Mid Strata - Shrub, 1.01-3m, Sparse. *Species includes - Petalostigma pubescens, Acacia species, Melaleuca species
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus melanophloia, Eucalyptus papuana
	Surface Coarse Fragments:	0-2%, medium gravelly, 6-20mm, subrounded, Sandstone
	Profile Morphology
	A11	0 - 0.15 m	Brown (10YR4/3-Moist); ; Loamy sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Dry; Very weak consistence; 0-2%, medium gravelly, 6-20mm, subangular, dispersed, 
	Sandstone, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); 
	Clear, Irregular change to - 
	A2e	0.15 - 0.3 m	Brown (10YR5/3-Moist); ; Sand; Massive grade of structure; Sandy (grains prominent) fabric; Dry;
	 2-10%, medium gravelly, 6-20mm, subangular, dispersed, Sandstone, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.2); Clear, Wavy change to - 
	D1	0.3 - 0.6 m	; Dry; Very weak consistence; 50-90%, cobbly, 60-200mm, subrounded, dispersed, Sandstone, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.6); Clear, Wavy 
	change to - 
	D2	0.6 - 0.7 m	; Coarse sand; Massive grade of structure; Sandy (grains prominent) fabric; Dry; Very weak 
	consistence; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1743	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1743	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile