Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	175	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	09/10/90	Elevation:	460 metres
	Map Ref.:	Sheet No. : 7959   GPS	Rainfall:	No Data
	Northing/Long.:	7897817 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	289763  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Detrital sedimentary 
	rock (unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	100 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol Thin Gravelly Clay-loamy 	Principal Profile Form:	Dr2.12
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Non-calcic brown 
	All necessary analytical data are available.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Heteropogon contortus, Themeda triandra, 
	Dichanthium sericeum	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus erythrophloia, Eucalyptus crebra
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus crebra, Eucalyptus papuana
	Surface Coarse Fragments:	10-20%, coarse gravelly, 20-60mm, rounded tabular, Detrital sedimentary rock (unidentified)
	Profile Morphology
	A1	0 - 0.05 m	Dark reddish brown (5YR3/3-Moist); ; Clay loam; Weak grade of structure, 10-20 mm, Subangular
	 blocky; Smooth-ped fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, Dry; Very firm 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Many, fine (1-2mm) 
	roots; Abrupt, Smooth change to - 
	B1	0.05 - 0.3 m	Reddish brown (5YR4/4-Moist); ; Medium clay; Strong grade of structure, 50-100 mm, Prismatic; 
	Strong grade of structure, 20-50 mm, Angular blocky; Smooth-ped fabric; Many (>5 per 100mm2) 
	Fine (1-2mm) macropores, Dry; Very firm consistence; 0-2%, fine gravelly, 2-6mm, angular, 
	dispersed, Detrital sedimentary rock (unidentified), coarse fragments; Few cutans, <10% of ped 
	faces or walls coated, prominent; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); 
	Many, fine (1-2mm) roots; Clear, Smooth change to - 
	B21t	0.3 - 0.55 m	Red (2.5YR4/6-Moist); ; Medium clay; Strong grade of structure, 20-50 mm, Prismatic; Strong 
	grade of structure, 10-20 mm, Subangular blocky; Smooth-ped fabric; Many (>5 per 100mm2) 
	Fine (1-2mm) macropores, Dry; Very firm consistence; 0-2%, fine gravelly, 2-6mm, angular, 
	dispersed, Detrital sedimentary rock (unidentified), coarse fragments; Many cutans, >50% of ped
	 faces or walls coated, prominent; , Calcareous, , ; , Gypseous, , ; Few, very fine (0-1mm) roots; 
	Abrupt, Smooth change to - 
	B31	0.55 - 0.62 m	; , Polyhedral; 90-100%, coarse gravelly, 20-60mm, angular, undisturbed, Detrital sedimentary 
	rock (unidentified), coarse fragments; , Calcareous, , ; , Gypseous, , ; Abrupt, Smooth change to
	 - 
	B32t	0.62 - 0.74 m	Brown (7.5YR4/4-Moist); ; Medium clay; Strong grade of structure, 10-20 mm; Smooth-ped fabric;
	 Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Moderately moist; Very firm 
	consistence; 0-2%, fine gravelly, 2-6mm, angular, dispersed, Detrital sedimentary rock 
	(unidentified), coarse fragments; Many cutans, >50% of ped faces or walls coated, prominent; , 
	Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 0.7); Clear, Smooth change to - 
	C	0.74 - 1.1 m	; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 1); 
	Morphological Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	175	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Notes
	Observation Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	175	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	7.1A	12B	8.5	0.67	0.05
	0.05 - 0.3	7A	12J	9.2	0.1	0.1	22.9I	0.44
	0.62 - 0.74	7.5A
	0.74 - 1	7.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.3
	0.62 - 0.74
	0.74 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.3
	0.62 - 0.74
	0.74 - 1

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	175	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension