Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1754	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	13/05/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8055   GPS	Rainfall:	No Data
	Northing/Long.:	7659776 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	396064  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Self-Mulching Brown Vertosol Non-gravelly Medium 	Principal Profile Form:	Ug5.28
	fine Medium fine Very deep 
	ASC Confidence:	Great Soil Group:	Grey clay
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Paspalidium species, Sporobolus caroli, 
	Dichanthium species	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Acacia harpophylla
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Casuarina cristata, Acacia harpophylla
	Surface Coarse Fragments:	2-10%, coarse gravelly, 20-60mm, subangular, Limestone
	Profile Morphology
	A11	0 - 0.05 m	Greyish brown (2.5Y5/2-Moist); ; Medium clay; Moderate grade of structure, 2-5 mm, Granular; 
	Rough-ped fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 9.5 
	(Raupach, 0.03); 
	B21	0.05 - 1.2 m	Greyish brown (2.5Y5/3-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ;
	 Field pH 9.9 (Raupach, 0.2); 
	B22	1.2 - 1.4 m	Greyish brown (2.5Y5/2-Moist); Mottles, 2.5Y53, 20-50% , 0-5mm, Faint; Mottles, 20-50% ; 
	Medium heavy clay; Moderate grade of structure, 10-20 mm, Subangular blocky; Smooth-ped 
	fabric; Moderately moist; Very firm consistence; Very few (0 - 2 %), , , ; , Calcareous, , ; , 
	Gypseous, , ; Field pH 9.9 (Raupach, 1.4); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1754	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1754	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile