Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1764	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Bright, J (Mitch)	Locality:
	Date Desc.:	23/07/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8155   GPS	Rainfall:	No Data
	Northing/Long.:	7656715 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	433486  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Sandstone 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached Eutrophic Brown Chromosol Thin Non-gravelly 	Principal Profile Form:	Dy4.43
	Sandy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, <0.25m, Sparse. *Species includes - Chrysopogon fallax, Cyperus species, Enteropogon 
	species	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Grevillea species
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus brownii, Eucalyptus melanophloia, Acacia 
	argyrodendron
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.08 m	Brown (7.5YR4/4-Moist); ; Loamy sand; Single grain grade of structure; Sandy (grains prominent)
	 fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 
	0.05); Gradual change to - 
	A12	0.08 - 0.3 m	Brown (10YR4/3-Moist); ; Loamy sand; Single grain grade of structure; Sandy (grains prominent) 
	fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.7 (Raupach, 0.2); 
	Gradual change to - 
	A13	0.3 - 0.6 m	Yellowish brown (10YR5/4-Moist); ; Clayey sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Weak consistence; 0-2%, medium gravelly, 6-20mm, rounded, Ironstone, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.4); Gradual change to
	 - 
	A2e	0.6 - 0.7 m	Light grey (10YR7/1-Moist); ; Clayey sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Very weak consistence; 10-20%, medium gravelly, 6-20mm, rounded, 
	Ironstone, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.65); 
	B2	0.7 - 1 m	Yellowish brown (10YR5/6-Moist); ; Light clay; , Calcareous, , ; , Gypseous, , ; Field pH 8.5 
	(Raupach, 0.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1764	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1764	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile