Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1794	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	07/06/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8255   GPS	Rainfall:	No Data
	Northing/Long.:	7629390 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	466778  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Sandstone 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Ridge	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting, Surface flake
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Eutrophic Red Chromosol     	Principal Profile Form:	Dy3.13
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Hummock grass, 0.51-1m, Mid-dense. *Species includes - Triodia mitchelii
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus shirleyi
	Surface Coarse Fragments:	2-10%, coarse gravelly, 20-60mm, subrounded, Sandstone
	Profile Morphology
	A11	0 - 0.1 m	Dark reddish brown (5YR3/4-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Dry; Weak consistence; 0-2%, medium gravelly, 6-20mm, angular, dispersed, Sandstone, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Clear change to -
	B21	0.1 - 0.21 m	Reddish brown (5YR4/4-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Angular 
	blocky; Smooth-ped fabric; Dry; Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field 
	pH 7 (Raupach, 0.15); Clear change to - 
	B22	0.21 - 0.35 m	Dark reddish grey (5YR4/2-Moist); Mottles, 5YR53, 2-10% , Faint; Mottles, 2-10% ; Medium heavy 
	clay; Moderate grade of structure, 10-20 mm, Angular blocky; Moderate grade of structure, 5-10 
	mm, Angular blocky; Smooth-ped fabric; Dry; Very strong consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 8.5 (Raupach, 0.3); 
	C	0.35 - 0.45 m	; , Calcareous, , ; , Gypseous, , ; Field pH 9 (Raupach, 0.45); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1794	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1794	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile