Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1810	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	25/05/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8255   GPS	Rainfall:	No Data
	Northing/Long.:	7659634 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	477762  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting, Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Supracalcic Mottled-Subnatric Grey Sodosol Thin Non-	Principal Profile Form:	Dy3.43
	gravelly Sandy Clayey Very deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Aristida species
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.08 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Massive grade of structure; Earthy fabric; Dry; Very 
	weak consistence; 0-2%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.05); 
	A12	0.08 - 0.4 m	Brown (10YR5/3-Moist); ; Sand; Massive grade of structure; Earthy fabric; Dry; Very weak 
	consistence; 0-2%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.3); 
	A2e	0.4 - 0.6 m	Light brownish grey (10YR6/2-Moist); ; Sand; Single grain grade of structure; Earthy fabric; Dry; 
	Very weak consistence; 0-2%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.5); 
	B21	0.6 - 0.9 m	Light brownish grey (10YR6/2-Moist); Mottles, 10YR68, 10-20% , 5-15mm, Prominent; Mottles, 
	10-20% ; Medium clay; Moderate grade of structure, 50-100 mm, Prismatic; Moderate grade of 
	structure, 20-50 mm, Angular blocky; Smooth-ped fabric; Dry; Very firm consistence; 0-2%, fine 
	gravelly, 2-6mm, rounded, dispersed, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; 
	Field pH 8 (Raupach, 0.75); 
	B22k	0.9 - 1.2 m	Brown (10YR5/3-Moist); ; Medium clay; Moderate grade of structure, 50-100 mm, Angular blocky; 
	Smooth-ped fabric; Dry; Strong consistence; 10-20%, medium gravelly, 6-20mm, rounded, 
	dispersed, Quartz, coarse fragments; Common (10 - 20 %), Manganiferous, Medium (2 -6 mm), 
	Nodules; Many (20 - 50 %), Calcareous, Fine (0 - 2 mm), ; , Gypseous, , ; Soil matrix is Highly 
	calcareous; Field pH 9.5 (Raupach, 1.2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1810	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1810	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile