Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	182	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	10/10/90	Elevation:	480 metres
	Map Ref.:	Sheet No. : 7860   GPS	Rainfall:	No Data
	Northing/Long.:	7909622 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	278500  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Low hills
	10%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Bleached-Leptic Tenosol Thin Non-gravelly 	Principal Profile Form:	Uc2.21
	Loamy Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Themeda triandra, Heteropogon contortus, 
	Bothriochloa decipiens	Mid Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus brownii
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Dark brown (10YR3/3-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Many (>5 
	per 100mm2) Fine (1-2mm) macropores, Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; 
	Field pH 6 (Raupach, 0.05); Few, very fine (0-1mm) roots; Clear, Smooth change to - 
	A21j	0.05 - 0.2 m	Brown (10YR4/3-Moist); ; Sandy loam (Heavy); Massive grade of structure; Earthy fabric; Many 
	(>5 per 100mm2) Fine (1-2mm) macropores, Dry; Firm consistence; , Calcareous, , ; , Gypseous,
	 , ; Few, very fine (0-1mm) roots; Abrupt, Smooth change to - 
	A22e	0.2 - 0.28 m	Yellowish brown (10YR5/4-Moist); ; Sandy clay loam (Light); Massive grade of structure; Earthy 
	fabric; Many (>5 per 100mm2) Medium (2-5mm) macropores, Dry; Firm consistence; , 
	Calcareous, , ; , Gypseous, , ; Few, very fine (0-1mm) roots; Abrupt, Smooth change to - 
	D1	0.28 - 0.5 m	Brownish yellow (10YR6/6-Moist); ; Clayey coarse sand; Single grain grade of structure; Earthy 
	fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, Dry; Loose consistence; 90-100%, 
	medium gravelly, 6-20mm, angular tabular, dispersed, Quartz, coarse fragments; , Calcareous, , 
	; , Gypseous, , ; Field pH 6.5 (Raupach, 0.3); Abrupt, Smooth change to - 
	D2	0.5 - 0.7 m	Strong brown (7.5YR5/6-Moist); ; Coarse sand; Single grain grade of structure; Earthy fabric; 
	Many (>5 per 100mm2) Fine (1-2mm) macropores, Dry; Loose consistence; 90-100%, fine 
	gravelly, 2-6mm, angular, dispersed, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; 
	Field pH 6.5 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	182	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.5A	6.1B	2.7	0.76	0.04
	0.28 - 0.5	6.4A	2.3J	1.8	0.4	0.1	4.2I	2.38
	0.5 - 0.7	6.7A	0.71B	0.87	0.12	0.07
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.28 - 0.5
	0.5 - 0.7
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.28 - 0.5
	0.5 - 0.7

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	182	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension