Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1822	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	26/05/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8255   GPS	Rainfall:	No Data
	Northing/Long.:	7652530 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	478789  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Self-Mulching Black Vertosol Slightly gravelly Fine 	Principal Profile Form:	Ug5.12
	Medium fine Moderately deep 
	ASC Confidence:	Great Soil Group:	Grey clay
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Mid Strata - , , . *Species includes - Terminalia oblongata, Acacia harpophylla
	Tall Strata - , , . *Species includes - None Recorded
	Surface Coarse Fragments:	2-10%, fine gravelly, 2-6mm, rounded, Quartz
	Profile Morphology
	A11	0 - 0.01 m	Very dark greyish brown (10YR3/2-Moist); ; Light medium clay; Massive grade of structure; 
	Smooth-ped fabric; Dry; Very weak consistence; 0-2%, fine gravelly, 2-6mm, rounded, dispersed,
	 Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.01); 
	A12	0.01 - 0.1 m	Dark grey (10YR4/1-Moist); ; Medium clay; Strong grade of structure, 5-10 mm, Angular blocky; 
	Smooth-ped fabric; Dry; Very weak consistence; 0-2%, fine gravelly, 2-6mm, rounded, dispersed,
	 Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.08); 
	B21	0.1 - 0.35 m	Very dark grey (2.5Y3/1-Moist); ; Medium clay; Strong grade of structure; Smooth-ped fabric; 
	Moderately moist; Strong consistence; 0-2%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, 
	coarse fragments; Common cutans, 10-50% of ped faces or walls coated, distinct; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.2); 
	B22	0.35 - 1 m	Black (2.5Y2/1-Moist); ; Medium clay; Strong grade of structure; Smooth-ped fabric; Moderately 
	moist; Strong consistence; 0-2%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, coarse 
	fragments; Common cutans, 10-50% of ped faces or walls coated, distinct; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7.5 (Raupach, 0.7); 
	BC	1 - 1.1 m	Grey (2.5Y5/1-Moist); ; Sandy medium clay; Massive grade of structure; Moderately moist; Strong
	 consistence; , Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1822	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1822	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile