Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1828	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	27/05/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8255   GPS	Rainfall:	No Data
	Northing/Long.:	7641130 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	488448  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Surface crust, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Crusty Grey Vertosol Gravelly Fine Medium fine 	Principal Profile Form:	Ug5.22
	Moderately deep 
	ASC Confidence:	Great Soil Group:	Grey clay
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Cenchrus ciliaris
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 3.01-6m, Sparse. *Species includes - Terminalia oblongata
	Surface Coarse Fragments:	10-20%, fine gravelly, 2-6mm, rounded, Quartz
	Profile Morphology
	A11	0 - 0.02 m	Dark greyish brown (10YR4/2-Moist); ; Silty light clay; Weak grade of structure, 2-5 mm, Granular;
	 Smooth-ped fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 
	(Raupach, 0.02); 
	A12	0.02 - 0.15 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Angular
	 blocky; Smooth-ped fabric; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 
	7 (Raupach, 0.1); 
	B21	0.15 - 0.6 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, 
	Angular blocky; Smooth-ped fabric; Dry; Very firm consistence; Common cutans, 10-50% of ped 
	faces or walls coated, distinct; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.5); 
	C	0.6 - 0.7 m	; Smooth-ped fabric; Dry; Very firm consistence; 50-90%, medium gravelly, 6-20mm, angular, 
	dispersed, Siltstone, coarse fragments; Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Soft 
	segregations; , Gypseous, , ; Soil matrix is Moderately calcareous; Field pH 8.5 (Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1828	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1828	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile