Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1831	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	27/05/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8255   GPS	Rainfall:	No Data
	Northing/Long.:	7637902 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	481711  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Gently inclined
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Self-mulching, Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Self-Mulching Black Vertosol Slightly gravelly Medium 	Principal Profile Form:	Ug5.14
	fine Very fine Very thick 
	ASC Confidence:	Great Soil Group:	Black earth
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:	2-10%, fine gravelly, 2-6mm, rounded, Basalt
	Profile Morphology
	A11	0 - 0.01 m	Very dark greyish brown (2.5Y3/2-Moist); ; Medium clay; Moderate grade of structure, 5-10 mm, 
	Granular; Smooth-ped fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field 
	pH 9.5 (Raupach, 0.01); 
	A12	0.01 - 0.18 m	Very dark greyish brown (2.5Y3/2-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 
	mm, Angular blocky; Smooth-ped fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, ,
	 ; Field pH 9 (Raupach, 0.15); 
	B2	0.18 - 1 m	Very dark greyish brown (10YR3/2-Moist); ; Medium heavy clay; Strong grade of structure, 50-100 
	mm, Lenticular; Strong grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; 
	Moderately moist; Very strong consistence; Many cutans, >50% of ped faces or walls coated, 
	distinct; Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Soft segregations; , Gypseous, , ; Field 
	pH 8.5 (Raupach, 0.3); 
	BC	1 - 1.7 m	; Medium heavy clay; Strong grade of structure; Earthy fabric; Moderately moist; Weak 
	consistence; Common (10 - 20 %), Calcareous, Medium (2 -6 mm), Soft segregations; , 
	Gypseous, , ; Field pH 8 (Raupach, 1.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1831	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1831	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile