Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1841	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	06/07/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8155   GPS	Rainfall:	No Data
	Northing/Long.:	7672304 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	415261  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Existing vertical exposure, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Red Dermosol     	Principal Profile Form:	Dr3.12
	ASC Confidence:	Great Soil Group:	No suitable group
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Eriachne species, Aristida species
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Hakea species, Ironbark, Bursaria incana
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus melanophloia, Eucalyptus erythrophloia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0.07 - 0.18 m	Strong brown (7.5YR4/6-Moist); ; Sandy clay loam (Light); Massive grade of structure; Earthy 
	fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.1); Clear
	 change to - 
	A12	0.18 - 0.3 m	Strong brown (7.5YR5/8-Moist); ; Clay loam, sandy (Heavy); Massive grade of structure; Earthy 
	fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.25); Clear 
	change to - 
	B21	0.3 - 0.5 m	Yellowish red (5YR5/8-Moist); Mottles, 5Y66, 2-10% , 5-15mm, Prominent; Mottles, 2-10% ; 
	Sandy medium clay; Weak grade of structure, 10-20 mm, Subangular blocky; Smooth-ped fabric;
	 Dry; Strong consistence; Very few (0 - 2 %), Ferromanganiferous, Fine (0 - 2 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.4); Gradual change to - 
	B22	0.5 - 0.95 m	Red (2.5YR4/8-Moist); Mottles, 5Y78, 10-20% , 15-30mm, Prominent; Mottles, 10-20% ; Sandy 
	medium clay; Moderate grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; Dry; 
	Very strong consistence; Very few (0 - 2 %), Ferromanganiferous, Fine (0 - 2 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.8); Gradual change to - 
	B23	0.95 - 1.2 m	Light brownish grey (10YR6/2-Moist); Mottles, 10YR68, 0-2% , 5-15mm, Prominent; Mottles, 
	2.5YR48, 0-2% ; Sandy medium heavy clay; Moderate grade of structure, 10-20 mm, Angular 
	blocky; Smooth-ped fabric; Dry; Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field 
	pH 7 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1841	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1841	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile