Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1846	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	06/07/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8155   GPS	Rainfall:	No Data
	Northing/Long.:	7676343 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	421766  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Siltstone 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hypocalcic Subnatric Brown Sodosol     	Principal Profile Form:	Db1.43
	ASC Confidence:	Great Soil Group:	Solodic soil
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Isolated plants. *Species includes - Unknown species, Unknown species, 
	Unknown species	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus brownii, Eucalyptus papuana
	Surface Coarse Fragments:	10-20%, coarse gravelly, 20-60mm, angular, 
	Profile Morphology
	A11	0 - 0.08 m	Dark brown (7.5YR3/4-Moist); ; Clay loam, fine sandy; Massive grade of structure; Earthy fabric; 
	Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Abrupt 
	change to - 
	A2e	0.08 - 0.1 m	Brown (7.5YR4/4-Moist); ; Fine sandy clay loam; Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.1); Sharp change 
	to - 
	B21	0.1 - 0.32 m	Dark brown (7.5YR3/4-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Very strong consistence; Very few (0 - 2 %), 
	Ferromanganiferous, Fine (0 - 2 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 8.5 
	(Raupach, 0.3); Gradual change to - 
	B22k	0.32 - 0.63 m	Strong brown (7.5YR4/6-Moist); ; Medium heavy clay; Moderate grade of structure, 10-20 mm, 
	Angular blocky; Smooth-ped fabric; Dry; Very strong consistence; Very few (0 - 2 %), 
	Ferromanganiferous, Fine (0 - 2 mm), Nodules; Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), 
	Soft segregations; , Gypseous, , ; Soil matrix is Highly calcareous; Field pH 8.5 (Raupach, 0.6); 
	Clear change to - 
	BC	0.63 - 0.9 m	Brown (7.5YR5/4-Moist); ; Medium clay; Weak grade of structure, 5-10 mm, Polyhedral; Smooth-
	ped fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Soil matrix is Slightly 
	calcareous; Field pH 8.5 (Raupach, 0.8); Field pH 8.5 (Raupach, 0.9); 
	C	0.9 - 0.95 m	; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1846	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1846	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile