Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1865	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	08/07/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8155   GPS	Rainfall:	No Data
	Northing/Long.:	7627856 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	430090  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Subnatric Grey Sodosol     	Principal Profile Form:	Dy2.43
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Hummock grass, 0.51-1m, Sparse. *Species includes - Triodia mitchelii
	Mid Strata - , , . *Species includes - Eucalyptus cambageana, Eremophila mitchellii
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus cambageana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.12 m	Dark brown (7.5YR3/3-Moist); ; Sandy clay loam; Massive grade of structure; Dry; Firm 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Field pH 6 (Raupach, 
	0.1); Clear change to - 
	A2e	0.12 - 0.14 m	Brown (7.5YR4/2-Moist); ; Sandy clay loam (Light); Massive grade of structure; Dry; Very strong 
	consistence; , Calcareous, , ; , Gypseous, , ; Abrupt change to - 
	B21	0.14 - 0.4 m	Dark greyish brown (10YR4/2-Moist); ; Sandy light clay; Dry; Rigid consistence; , Calcareous, , ; 
	, Gypseous, , ; Field pH 8.5 (Raupach, 0.3); 
	B22	0.4 - 0.5 m	Brown (10YR4/3-Moist); ; Sandy light clay; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 8.5 
	(Raupach, 0.5); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1865	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1865	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile