Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	187	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	07/08/90	Elevation:	255 metres
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7730374 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	418908  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	140 degrees
	Surface Soil Condition (dry):	Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Subnatric Yellow Sodosol Medium Non-gravelly 	Principal Profile Form:	Db1.13
	Clay-loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data and little or no knowledge of this soil.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Sporobolus caroli, Bothriochloa ewartiana
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eremophila mitchellii, Lysiphillum carronii, Acacia harpophylla
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Acacia harpophylla, Eucalyptus cambageana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (10YR3/3-Moist); ; Clay loam, fine sandy; Strong grade of structure, 2-5 mm, 
	Granular; Smooth-ped fabric; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field 
	pH 6.5 (Raupach, 0.05); Many, fine (1-2mm) roots; Abrupt, Smooth change to - 
	B21	0.1 - 0.35 m	Brown (10YR4/3-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, Angular 
	blocky; Strong grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; Moderately 
	moist; Firm consistence; Few cutans, <10% of ped faces or walls coated, distinct; Few (2 - 10 
	%), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 9.9 
	(Raupach, 0.3); Many, fine (1-2mm) roots; Clear, Smooth change to - 
	B22	0.35 - 1.7 m	Dark yellowish brown (10YR4/4-Moist); ; Medium clay; Strong grade of structure, 20-50 mm, 
	Lenticular; Strong grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; Moist; Firm 
	consistence; Common cutans, 10-50% of ped faces or walls coated, distinct; Few (2 - 10 %), 
	Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 9.9 
	(Raupach, 0.9); Common, fine (1-2mm) roots; Gradual, Smooth change to - 
	B23	1.7 - 2.1 m	Dark yellowish brown (10YR4/4-Moist); Mottles, 10YR56, 2-10% , 5-15mm, Faint; Mottles, 2-10% 
	; Medium clay; Smooth-ped fabric; Moist; Firm consistence; Common cutans, 10-50% of ped 
	faces or walls coated, distinct; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; Field pH 9.9 (Raupach, 1.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	187	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.4A
	0.1 - 0.35	8.9A
	0.35 - 1.7	8.8A	6.5E	7.3	0.32	6.9	21B	32.86
	1.7 - 2.1	8.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.35
	0.35 - 1.7
	1.7 - 2.1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.35
	0.35 - 1.7
	1.7 - 2.1

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	187	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, 
	pretreatment for soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	4A1	pH of 1:5 soil/water suspension