Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1881	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	08/09/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7958   GPS	Rainfall:	No Data
	Northing/Long.:	7831640 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	304481  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Self-Mulching Black Vertosol     	Principal Profile Form:	Ug5.1
	ASC Confidence:	Great Soil Group:	Black earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Isolated plants. *Species includes - None recorded
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus orgadophylla
	Surface Coarse Fragments:	0-2%, stony, 200-600mm, subrounded, Basalt
	Profile Morphology
	A11	0 - 0.03 m	Black (7.5YR2/0-Moist); ; Medium clay; Strong grade of structure, 2-5 mm, Granular; Rough-ped 
	fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.02); 
	Abrupt change to - 
	A12	0.03 - 0.3 m	Black (7.5YR2/0-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Rigid consistence; , Calcareous, , ; , Gypseous, , ; 
	Field pH 6.5 (Raupach, 0.25); Gradual change to - 
	B21	0.3 - 0.6 m	Black (7.5YR2/0-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, Lenticular; 
	Moderate grade of structure, 10-20 mm, Subangular blocky; Smooth-ped fabric; Moderately 
	moist; Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.5); 
	Gradual change to - 
	B22	0.6 - 0.9 m	Black (7.5YR2/0-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, Lenticular; 
	Moderate grade of structure, 10-20 mm, Subangular blocky; Smooth-ped fabric; Moderately 
	moist; Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 0.8); 
	Gradual change to - 
	BC	0.9 - 1 m	Black (7.5YR2/0-Moist); ; Medium heavy clay; Massive grade of structure; Smooth-ped fabric; 
	Dry; Strong consistence; 20-50%, coarse gravelly, 20-60mm, subangular, Basalt, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 9 (Raupach, 1); 
	C	1 - 1.1 m	Yellowish brown (10YR5/6-Moist); ; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 9 (Raupach, 
	1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1881	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1881	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile