Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	190	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	19/09/90	Elevation:	305 metres
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	7811798 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	383464  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Basalt 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):	Cracking, Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endocalcareous Epipedal Black Vertosol Non-gravelly 	Principal Profile Form:	Ug5.13
	Medium fine Very fine Moderately deep 
	ASC Confidence:	Great Soil Group:	Black earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Mid-dense. *Species includes - Bothriochloa ewartiana, Bothriochloa bladhii
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus brownii, Acacia farnesiana
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus brownii, Eucalyptus papuana
	Surface Coarse Fragments:	0-2%, fine gravelly, 2-6mm, rounded, Quartz
	Profile Morphology
	A1	0 - 0.05 m	Very dark grey (10YR3/1-Moist); ; Medium clay; Strong grade of structure, 5-10 mm, Granular; 
	Smooth-ped fabric; Coarse, (10 - 20) mm crack; Dry; Very firm consistence; 10-20%, fine 
	gravelly, 2-6mm, rounded, dispersed, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; 
	Field pH 6 (Raupach, 0.05); Common, fine (1-2mm) roots; Clear, Smooth change to - 
	B21	0.05 - 0.8 m	Very dark grey (10YR3/1-Moist); ; Heavy clay; Strong grade of structure, 20-50 mm, Angular 
	blocky; Smooth-ped fabric; Moderately moist; Strong consistence; 10-20%, fine gravelly, 2-6mm,
	 rounded, dispersed, Quartz, coarse fragments; Few cutans, <10% of ped faces or walls coated,
	 prominent; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.6); Few, very fine (0-1mm) 
	roots; Clear, Smooth change to - 
	B22	0.8 - 0.95 m	Very dark greyish brown (2.5Y3/2-Moist); ; Heavy clay; Very few (0 - 2 %), Calcareous, Medium (2 
	-6 mm), Nodules; , Gypseous, , ; Field pH 8.5 (Raupach, 0.95); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	190	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.3A
	0.05 - 0.8	7.9A
	0.8 - 0.95	8.3A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.8
	0.8 - 0.95
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.8
	0.8 - 0.95

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	190	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension