Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1909	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	25/05/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8255   GPS	Rainfall:	No Data
	Northing/Long.:	7659109 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	482756  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Self-Mulching Brown Vertosol Gravelly Medium fine 	Principal Profile Form:	Ug
	Very fine Deep 
	ASC Confidence:	Great Soil Group:	Brown clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Cenchrus ciliaris
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Shrub, 1.01-3m, Sparse. *Species includes - Terminalia oblongata, Acacia argyrodendron
	Surface Coarse Fragments:	10-20%, coarse gravelly, 20-60mm, subrounded, Sandstone
	Profile Morphology
	A1	0 - 0.05 m	Dark yellowish brown (10YR4/4-Moist); ; Light medium clay; Moderate grade of structure, 10-20 
	mm, Subangular blocky; Smooth-ped fabric; Dry; Strong consistence; Very few (0 - 2 %), 
	Manganiferous, Medium (2 -6 mm), Soft segregations; , Calcareous, , ; , Gypseous, , ; Field pH 
	7.5 (Raupach, 0.02); Clear change to - 
	B1	0.05 - 0.25 m	Yellowish brown (10YR5/4-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Strong consistence; 0-2%, fine gravelly, 2-6mm, 
	subrounded, Quartz, coarse fragments; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Soft 
	segregations; , Calcareous, , ; , Gypseous, , ; Field pH 8.5 (Raupach, 0.15); Clear change to - 
	B21	0.25 - 0.85 m	Dark yellowish brown (10YR4/4-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 
	mm, Angular blocky; Moderate grade of structure, 5-10 mm, Subangular blocky; Smooth-ped 
	fabric; Moderately moist; Strong consistence; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm),
	 Soft segregations; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.6); Gradual change
	 to - 
	B22	0.85 - 1.7 m	Dark yellowish brown (10YR4/6-Moist); ; Medium heavy clay; Moderate grade of structure, 10-20 
	mm, Lenticular; Smooth-ped fabric; Moderately moist; Strong consistence; Few (2 - 10 %), 
	Manganiferous, Medium (2 -6 mm), Soft segregations; , Calcareous, , ; , Gypseous, , ; Field pH 6
	 (Raupach, 1.4); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1909	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1909	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile