Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1912	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	25/05/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8255   GPS	Rainfall:	No Data
	Northing/Long.:	7659057 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	486016  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous Self-Mulching Grey Vertosol Gravelly Medium 	Principal Profile Form:	Ug
	fine Very fine Deep 
	ASC Confidence:	Great Soil Group:	Grey clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Cenchrus ciliaris
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Shrub, 1.01-3m, Sparse. *Species includes - Terminalia oblongata, Atalaya hemiglauca
	Surface Coarse Fragments:	10-20%, coarse gravelly, 20-60mm, subrounded, Quartz
	Profile Morphology
	A	0 - 0.18 m	Greyish brown (2.5Y5/2-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Polyhedral; 
	Smooth-ped fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 
	(Raupach, 0.1); 
	B1	0.18 - 0.4 m	Greyish brown (2.5Y5/2-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 mm, 
	Subangular blocky; Moderate grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; 
	Dry; Strong consistence; Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), ; , Gypseous, , ; Soil 
	matrix is Moderately calcareous; Field pH 9 (Raupach, 0.3); 
	B21	0.4 - 0.9 m	Greyish brown (2.5Y5/2-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, 
	Angular blocky; Smooth-ped fabric; Moderately moist; Strong consistence; Very few (0 - 2 %), 
	Calcareous, Fine (0 - 2 mm), ; , Gypseous, , ; Soil matrix is Moderately calcareous; Field pH 9 
	(Raupach, 0.9); 
	B22	0.9 - 1.5 m	Light brownish grey (2.5Y6/2-Moist); Mottles, 7.5YR32, 10-20% , 0-5mm, Distinct; Mottles, 10-
	20% ; Medium heavy clay; Moderate grade of structure, 10-20 mm, Subangular blocky; Smooth-
	ped fabric; Moderately moist; Very firm consistence; Common (10 - 20 %), Manganiferous, 
	Medium (2 -6 mm), Soft segregations; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 
	1.5); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1912	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1912	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile