Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	194	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	08/04/91	Elevation:	290 metres
	Map Ref.:	Sheet No. : 8258   GPS	Rainfall:	No Data
	Northing/Long.:	7796011 AMG zone: 55	Runoff:	Very rapid
	Easting/Lat.:	454854  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Subnatric Yellow Sodosol Medium Slightly 	Principal Profile Form:	Dy3.23
	gravelly Sandy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Bothriochloa pertusa, Heteropogon contortus, 
	Eragrostis species	Mid Strata - Tree, 1.01-3m, Isolated plants. *Species includes - Albizia basaltica
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana
	Surface Coarse Fragments:	2-10%, cobbly, 60-200mm, subangular, Quartz
	Profile Morphology
	A2	0 - 0.15 m	Dark greyish brown (10YR4/2-Moist); ; Loamy sand; Massive grade of structure; Earthy fabric; 
	Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Very firm consistence; 0-2%, 
	fine gravelly, 2-6mm, subangular, dispersed, Granodiorite, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 5.5 (Raupach, 0.05); Few, very fine (0-1mm) roots; Abrupt, Smooth 
	change to - 
	B21	0.15 - 0.5 m	Brownish yellow (10YR6/8-Moist); Mottles, 7.5YR33, 20-50% , 5-15mm, Distinct; Mottles, 20-
	50% ; Light medium clay; Strong grade of structure, 20-50 mm, Angular blocky; Smooth-ped 
	fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Strong consistence; 2-
	10%, medium gravelly, 6-20mm, angular, dispersed, Granodiorite, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	194	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	5.7A
	0.15 - 0.5	6.6A	4.4J	5.6	0.1	1.5	14.2I	10.56
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15
	0.15 - 0.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.5

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	194	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension