Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1948	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Bright, J (Mitch)	Locality:
	Date Desc.:	21/09/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7858   GPS	Rainfall:	No Data
	Northing/Long.:	7837071 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	237971  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Graywacke 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Hills
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol Thin Very gravelly Clay-	Principal Profile Form:	Dr2.12
	loamy Clayey Shallow
	ASC Confidence:	Great Soil Group:	Non-calcic brown 
	No analytical data are available but confidence is fair.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Themeda triandra, Chrysopogon fallax
	Mid Strata - Tree, 1.01-3m, Isolated clumps. *Species includes - Eucalyptus crebra
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	50-90%, cobbly, 60-200mm, angular, Graywacke
	Profile Morphology
	A1	0 - 0.08 m	Dark brown (10YR3/3-Moist); ; Fine sandy clay loam; Massive grade of structure; Earthy fabric; 
	Dry; Very weak consistence; 50-90%, medium gravelly, 6-20mm, angular, Graywacke, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Sharp change to - 
	B21	0.08 - 0.2 m	Red (2.5YR4/6-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Moderately moist; Weak consistence; , Calcareous, , ; , Gypseous, , 
	; Field pH 5.5 (Raupach, 0.15); Gradual change to - 
	B22	0.2 - 0.45 m	Brown (10YR4/3-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Subangular blocky; 
	Strong grade of structure, 5-10 mm, Angular blocky; Smooth-ped fabric; Moderately moist; Firm 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.3); 
	C	0.45 - 0.55 m	; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1948	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1948	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile