Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1966	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	05/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7857   GPS	Rainfall:	No Data
	Northing/Long.:	7759026 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	278377  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Schist 
	Land Form
	Rel/Slope Class: 	Rolling rises 9-30m 10-32%	Pattern Type:	Low hills
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Gently inclined
	Slope:	8 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Lithic Paralithic Orthic Tenosol Thick Gravelly Loamy Clay-	Principal Profile Form:	Uc5.23
	loamy Deep
	ASC Confidence:	Great Soil Group:	No suitable group
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Themeda triandra, Aristida species, Heteropogon 
	contortus	Mid Strata - Shrub, 1.01-3m, Very sparse. *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	2-10%, coarse gravelly, 20-60mm, angular, Quartz
	Profile Morphology
	A11	0 - 0.13 m	Very dark greyish brown (10YR3/2-Moist); ; Fine sandy loam; Massive grade of structure; Earthy 
	fabric; Dry; Firm consistence; 20-50%, coarse gravelly, 20-60mm, Substrate material, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 0.05); Clear change to - 
	A12	0.13 - 0.4 m	Dark greyish brown (10YR4/2-Moist); ; Fine sandy loam; Massive grade of structure; Earthy 
	fabric; Dry; Very weak consistence; 20-50%, coarse gravelly, 20-60mm, Substrate material, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); Gradual change to
	 - 
	0.4 - 0.5 m	Brown (10YR5/3-Moist); ; Fine sandy loam; Massive grade of structure; Earthy fabric; Very weak 
	consistence; 20-50%, coarse gravelly, 20-60mm, Substrate material, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.5); 
	B2	0.5 - 1.1 m	Olive (5Y5/3-Moist); ; Fine sandy clay loam (Heavy); Massive grade of structure; Dry; Very weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 9.5 (Raupach, 1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1966	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1966	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile