Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1982	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	07/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7858   GPS	Rainfall:	No Data
	Northing/Long.:	7814834 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	235989  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	7 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Eutrophic Brown Chromosol Thick Gravelly 	Principal Profile Form:	Dy3.43
	Loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Heteropogon contortus, Themeda triandra
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus crebra, Petalostigma pubescens
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	10-20%, fine gravelly, 2-6mm, subangular, Quartz
	Profile Morphology
	A11	0 - 0.08 m	Very dark greyish brown (10YR3/2-Moist); ; Sandy loam; Massive grade of structure; Earthy 
	fabric; Dry; Firm consistence; 0-2%, fine gravelly, 2-6mm, subrounded, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.04); Clear change to - 
	A12	0.08 - 0.19 m	Brown (10YR5/3-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; Firm 
	consistence; 0-2%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , Calcareous, , 
	; , Gypseous, , ; Field pH 6 (Raupach, 0.15); Clear change to - 
	A13	0.19 - 0.3 m	Light yellowish brown (10YR6/4-Moist); ; Coarse sandy clay loam; Massive grade of structure; 
	Earthy fabric; Dry; Firm consistence; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.25); Clear change to - 
	A2e	0.3 - 0.42 m	Light yellowish brown (10YR6/4-Moist); ; Coarse sandy clay loam (Light); Massive grade of 
	structure; Earthy fabric; Dry; Firm consistence; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz,
	 coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.4); Abrupt change to 
	- 
	B21	0.42 - 0.6 m	Brown (10YR5/3-Moist); Mottles, 10YR46, 10-20% , 5-15mm, Distinct; Mottles, 10-20% ; Light 
	medium clay; Moderate grade of structure, 20-50 mm, Angular blocky; Smooth-ped fabric; Dry; 
	Strong consistence; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.5); Clear change to - 
	B22	0.6 - 0.9 m	Dark yellowish brown (10YR4/6-Moist); Mottles, 10YR53, 2-10% , 5-15mm, Distinct; Mottles, 2-
	10% ; Sandy medium clay; Moderate grade of structure, 20-50 mm, Subangular blocky; Smooth-
	ped fabric; Dry; Strong consistence; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse 
	fragments; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Soft segregations; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.8); 
	B23	0.9 - 1.3 m	Dark yellowish brown (10YR4/6-Moist); ; Clay loam, sandy; , Calcareous, , ; , Gypseous, , ; Field 
	pH 8.5 (Raupach, 1.2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1982	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1982	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1982	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile