Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1984	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	07/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7858   GPS	Rainfall:	No Data
	Northing/Long.:	7789328 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	273427  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Brown Chromosol Thick Slightly gravelly 	Principal Profile Form:	Dy3.22
	Loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Themeda triandra, Chrysopogon fallax, Heteropogon 
	contortus	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus crebra
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	2-10%, medium gravelly, 6-20mm, subangular platy, Quartz
	Profile Morphology
	A11	0 - 0.1 m	Dark brown (10YR3/3-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; Firm 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Clear change to - 
	A12	0.1 - 0.2 m	Dark yellowish brown (10YR4/4-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; 
	Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.15); Clear 
	change to - 
	A13	0.2 - 0.3 m	Dark yellowish brown (10YR4/4-Moist); ; Sandy clay loam (Light); Massive grade of structure; 
	Sandy (grains prominent) fabric; Dry; Firm consistence; 20-50%, coarse gravelly, 20-60mm, 
	angular, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.25); 
	Abrupt change to - 
	B21	0.3 - 0.6 m	Light olive brown (2.5Y5/4-Moist); Mottles, 10YR56, 10-20% , 5-15mm, Prominent; Mottles, 10-
	20% ; Light medium clay; Moderate grade of structure, 20-50 mm, Subangular blocky; Dry; 
	Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.5); 
	B22	0.6 - 1.1 m	Light olive brown (2.5Y5/4-Moist); ; , Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1984	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1984	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile