Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1988	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	09/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7858   GPS	Rainfall:	No Data
	Northing/Long.:	7807572 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	286407  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Manganic Eutrophic Brown Ferrosol Thin Slightly gravelly 	Principal Profile Form:	Gn3.12
	Clay-loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Euchrozem
	No analytical data are available but confidence is fair.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Themeda triandra, Chrysopogon fallax
	Mid Strata - Tree, 3.01-6m, Isolated clumps. *Species includes - Eucalyptus papuana
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus papuana, Eucalyptus crebra
	Surface Coarse Fragments:	2-10%, fine gravelly, 2-6mm, rounded, 
	Profile Morphology
	A1	0 - 0.06 m	Dark brown (10YR3/3-Moist); ; Clay loam; Moderate grade of structure, 2-5 mm, Polyhedral; 
	Smooth-ped fabric; Dry; Firm consistence; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm),
	 Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.03); Clear change to - 
	B21	0.06 - 0.23 m	Dark brown (7.5YR3/3-Moist); ; Light clay; Moderate grade of structure, 5-10 mm, Polyhedral; 
	Smooth-ped fabric; Dry; Very firm consistence; Few (2 - 10 %), Manganiferous, Medium (2 -6 
	mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.15); Clear change to - 
	B22	0.23 - 0.45 m	Dark brown (7.5YR3/4-Moist); ; Light clay; Moderate grade of structure, 5-10 mm, Polyhedral; 
	Smooth-ped fabric; Dry; Firm consistence; Common (10 - 20 %), Manganiferous, Medium (2 -6 
	mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.3); Clear change to - 
	B23	0.45 - 0.8 m	Strong brown (7.5YR4/6-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Polyhedral; 
	Smooth-ped fabric; Dry; Firm consistence; Many (20 - 50 %), Manganiferous, Medium (2 -6 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1988	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1988	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile