Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1994	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	19/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7959   GPS	Rainfall:	No Data
	Northing/Long.:	7885312 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	310772  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Manganic Eutrophic Brown Chromosol Thick Slightly gravelly 	Principal Profile Form:	N/A
	Clay-loamy Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	No suitable group
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Isolated plants. *Species includes - Unknown species, Unknown species, 
	Unknown species	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus brownii
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	2-10%, fine gravelly, 2-6mm, angular, Sandstone
	Profile Morphology
	A11	0 - 0.06 m	Brown (10YR4/3-Moist); ; Sandy clay loam (Light); Massive grade of structure; Earthy fabric; Dry; 
	Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.03); Clear change 
	to - 
	A12	0.06 - 0.3 m	Yellowish brown (10YR5/4-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; 
	Firm consistence; Common (10 - 20 %), Ferromanganiferous, Coarse (6 - 20 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.2); Clear change to - 
	B1	0.3 - 0.45 m	Light olive brown (2.5Y5/4-Moist); Mottles, 7.5YR58, 2-10% , 0-5mm, Faint; Mottles, 2-10% ; 
	Sandy loam; Massive grade of structure; Earthy fabric; Dry; Very firm consistence; Many (20 - 50 
	%), Ferromanganiferous, Coarse (6 - 20 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Duripan, 
	Strongly cemented, Massive; Field pH 6 (Raupach, 0.4); Clear change to - 
	B21	0.45 - 0.7 m	Yellowish brown (10YR5/4-Moist); ; Clay loam, sandy; Dry; 10-20%, medium gravelly, 6-20mm, 
	subrounded, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 
	0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1994	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1994	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile