Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2012	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Bright, J (Mitch)	Locality:
	Date Desc.:	09/06/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8255   GPS	Rainfall:	No Data
	Northing/Long.:	7623937 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	475076  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Self-mulching, Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Episodic-Epicalcareous Self-Mulching Brown Vertosol Non-	Principal Profile Form:	Ug5.25
	gravelly Fine Medium fine Deep 
	ASC Confidence:	Great Soil Group:	Grey clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Cenchrus ciliaris
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Shrub, 1.01-3m, Very sparse. *Species includes - Acacia species, Phebalium glandulosum
	Surface Coarse Fragments:	0-2%, coarse gravelly, 20-60mm, subrounded, Ironstone
	Profile Morphology
	A1	0 - 0.1 m	Very pale brown (10YR8/3-Moist); ; Light clay; Moderate grade of structure, <2 mm, Granular; 
	Smooth-ped fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Soil matrix is 
	Highly calcareous; Field pH 9 (Raupach, 0.05); Clear change to - 
	B21	0.1 - 0.5 m	Brown (10YR5/3-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Polyhedral; 
	Smooth-ped fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Soil matrix is 
	Highly calcareous; Field pH 9 (Raupach, 0.4); 
	B22	0.5 - 1.2 m	Dark yellowish brown (10YR4/4-Moist); Mottles, 10YR52, 20-50% , 5-15mm, Faint; Mottles, 20-
	50% ; Medium clay; Moderate grade of structure, 10-20 mm, Polyhedral; Smooth-ped fabric; Dry; 
	Strong consistence; Few (2 - 10 %), Calcareous, Fine (0 - 2 mm), Soft segregations; , 
	Gypseous, , ; Soil matrix is Highly calcareous; Field pH 9 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2012	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2012	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile