Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2016	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	09/06/93	Elevation:	180 metres
	Map Ref.:	Sheet No. : 8254   GPS	Rainfall:	No Data
	Northing/Long.:	7610365 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	467510  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Mudstone 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Eutrophic Black Dermosol Medium Non-gravelly Clayey 	Principal Profile Form:	Uf6.42
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Brown clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Heteropogon contortus, Bothriochloa species
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus erythrophloia, Eucalyptus brownii, 
	Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.25 m	Very dark grey (10YR3/1-Moist); ; Light medium clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Smooth-ped fabric; Dry; Very strong consistence; , Calcareous, , ; , Gypseous, , 
	; Field pH 6.5 (Raupach, 0.1); Gradual change to - 
	B21	0.25 - 0.7 m	Very dark greyish brown (10YR3/2-Moist); Mottles, 5YR58, 20-50% , 15-30mm, Distinct; Mottles, 
	20-50% ; Medium clay; Moderate grade of structure, 10-20 mm, Angular blocky; Smooth-ped 
	fabric; Dry; Very strong consistence; 0-2%, medium gravelly, 6-20mm, subangular, Mudstone, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 0.5); Gradual change to
	 - 
	B22	0.7 - 0.8 m	Dark brown (7.5YR3/3-Moist); ; Medium clay; Smooth-ped fabric; Dry; 0-2%, medium gravelly, 6-
	20mm, subangular, Mudstone, coarse fragments; , Calcareous, , ; , Gypseous, , ; 
	C	0.8 - 0.9 m	; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2016	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2016	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile