Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2021	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	10/06/93	Elevation:	320 metres
	Map Ref.:	Sheet No. : 8255   GPS	Rainfall:	No Data
	Northing/Long.:	7635974 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	471814  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Mudstone 
	Land Form
	Rel/Slope Class: 	Undulating hills 90-300m 3-	Pattern Type:	Hills
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm, Surface flake
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Eutrophic Brown Chromosol Medium Very gravelly 	Principal Profile Form:	Db1.13
	Loamy Clayey Shallow
	ASC Confidence:	Great Soil Group:	No suitable group
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, <0.25m, Very sparse. *Species includes - Aristida species
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eremophila mitchellii, Acacia ??? (from WARLUS V), 
	Erythroxylon australe
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Acacia ??? (from WARLUS V), Eucalyptus thozetiana
	Surface Coarse Fragments:	50-90%, medium gravelly, 6-20mm, angular, Sandstone
	Profile Morphology
	A1	0 - 0.1 m	Brown (7.5YR5/4-Moist); ; Fine sandy loam; Massive grade of structure; Earthy fabric; Dry; Very 
	firm consistence; 10-20%, coarse gravelly, 20-60mm, subangular, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Abrupt change to - 
	B21	0.1 - 0.2 m	Brown (7.5YR5/4-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 
	6.5 (Raupach, 0.15); Clear change to - 
	B22	0.2 - 0.35 m	Strong brown (7.5YR4/6-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ;
	 Field pH 7.5 (Raupach, 0.25); Gradual change to - 
	BC	0.35 - 0.5 m	Brown (7.5YR5/4-Moist); ; Light medium clay; Weak grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Dry; Very firm consistence; 20-50%, coarse gravelly, 20-60mm, 
	angular, Mudstone, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 9 (Raupach, 
	0.4); Gradual change to - 
	C	0.5 - 0.7 m	; , Calcareous, , ; , Gypseous, , ; Field pH 9 (Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2021	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2021	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile