Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2029	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	11/06/93	Elevation:	210 metres
	Map Ref.:	Sheet No. : 8255   GPS	Rainfall:	No Data
	Northing/Long.:	7642053 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	453820  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating hills 90-300m 3-	Pattern Type:	Hills
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Regolithic Calcic Calcarosol Slightly gravelly Clayey 	Principal Profile Form:	Uf6.31
	Medium Clayey Deep
	ASC Confidence:	Great Soil Group:	No suitable group
	No analytical data and little or no knowledge of this soil.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Bothriochloa ewartiana, Dichanthium sericeum, 
	Iseilema vaginiflorum	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Terminalia oblongata
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Acacia cambagei, Eucalyptus cambageana
	Surface Coarse Fragments:	2-10%, fine gravelly, 2-6mm, angular, 
	Profile Morphology
	A1	0 - 0.1 m	Brown (7.5YR4/3-Moist); ; Light clay; Weak grade of structure, 20-50 mm, Subangular blocky; 
	Rough-ped fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 
	0.05); Clear change to - 
	B21	0.1 - 0.45 m	Brown (7.5YR4/3-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Polyhedral; 
	Smooth-ped fabric; Dry; Strong consistence; Few (2 - 10 %), Calcareous, Fine (0 - 2 mm), 
	Nodules; , Gypseous, , ; Soil matrix is Slightly calcareous; Field pH 8.5 (Raupach, 0.3); Gradual
	 change to - 
	B22	0.45 - 0.8 m	Strong brown (7.5YR4/6-Moist); ; Light medium clay; Moderate grade of structure, 10-20 mm, 
	Polyhedral; Moderate grade of structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Dry; Firm 
	consistence; Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Nodules; , Gypseous, , ; Soil 
	matrix is Slightly calcareous; Field pH 8.5 (Raupach, 0.6); Gradual change to - 
	B23	0.8 - 1.1 m	Strong brown (7.5YR4/6-Moist); ; Light medium clay; Weak grade of structure, 5-10 mm, 
	Granular; Smooth-ped fabric; Dry; Very weak consistence; Few (2 - 10 %), Manganiferous, Fine 
	(0 - 2 mm), Soft segregations; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2029	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2029	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile