Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	203	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	09/04/91	Elevation:	270 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7787108 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	456592  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	Level
	Slope:	0 % 	Aspect:	100 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Orthic Tenosol Medium Non-gravelly Loamy 	Principal Profile Form:	Uc5.21
	Clay-loamy Deep
	ASC Confidence:	Great Soil Group:	Earthy sand
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Bothriochloa ewartiana, Chrysopogon fallax, 
	Heteropogon contortus	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus erythrophloia, Eucalyptus crebra, Eucalyptus 
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.12 m	Very dark greyish brown (10YR3/2-Moist); ; Sandy loam; Massive grade of structure; Earthy 
	fabric; Many (>5 per 100mm2) Coarse (>5mm) macropores, Dry; Very firm consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Common, medium (2-5mm) roots; 
	Gradual, Smooth change to - 
	B2	0.12 - 0.5 m	Dark brown (10YR3/3-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Many (>5 
	per 100mm2) Medium (2-5mm) macropores, Dry; Firm consistence; , Calcareous, , ; , Gypseous,
	 , ; Field pH 6.5 (Raupach, 0.3); Common, medium (2-5mm) roots; Gradual, Smooth change to - 
	D	0.5 - 0.95 m	Yellowish red (5YR3/6-Moist); ; Coarse sandy clay loam; Massive grade of structure; Smooth-
	ped fabric; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Moist; Firm consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.6); Few, very fine (0-1mm) roots; Clear, 
	Smooth change to - 
	A1b	0.95 - 1.15 m	Dark brown (7.5YR3/3-Moist); ; Coarse sand; Massive grade of structure; Earthy fabric; Many (>5 
	per 100mm2) Fine (1-2mm) macropores, Wet; Very weak consistence; , Calcareous, , ; , 
	Gypseous, , ; Gradual, Smooth change to - 
	A2b	1.15 - 1.45 m	Reddish brown (5YR4/3-Moist); ; Coarse sand; Massive grade of structure; Earthy fabric; Many 
	(>5 per 100mm2) Fine (1-2mm) macropores, Wet; Very weak consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 9 (Raupach, 1.2); 
	B21b	1.45 - 1.5 m	; Clayey coarse sand; Moderate grade of structure, 10-20 mm, Angular blocky; Smooth-ped 
	fabric; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Wet; Weak consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 1.5); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	203	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	6.8A
	0.12 - 0.5	6.8A	4J	3.1	0.1	0.3	8.9I	3.37
	0.5 - 0.95	6.9A
	1.15 - 1.45	7.7A
	1.45 - 1.5	8.8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12
	0.12 - 0.5
	0.5 - 0.95
	1.15 - 1.45
	1.45 - 1.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.12 - 0.5
	0.5 - 0.95
	1.15 - 1.45
	1.45 - 1.5

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	203	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension