Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2031	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	21/06/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8255   GPS	Rainfall:	No Data
	Northing/Long.:	7670086 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	449295  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Black Dermosol Thin Non-gravelly Clay-	Principal Profile Form:	Gn3.32
	loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	No suitable group
	No analytical data are available but confidence is fair.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None recorded
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus coolibah
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Eucalyptus coolibah, Eucalyptus polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.04 m	Very dark greyish brown (10YR3/2-Moist); ; Clay loam; Weak grade of structure, 2-5 mm, Platy; 
	Smooth-ped fabric; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.02); Abrupt change to - 
	A2j	0.04 - 0.26 m	Dark grey (10YR4/1-Moist); ; Fine sandy light clay; Weak grade of structure, 2-5 mm, Platy; 
	Smooth-ped fabric; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Strong 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.15); Clear change to - 
	B21	0.26 - 0.4 m	Very dark greyish brown (10YR3/2-Moist); ; Medium clay (Light); Moderate grade of structure, 20-
	50 mm, Subangular blocky; Smooth-ped fabric; Dry; Strong consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6 (Raupach, 0.4); Gradual change to - 
	B22	0.4 - 1.5 m	Brown (10YR5/3-Moist); ; Light medium clay; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 8 
	(Raupach, 1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2031	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2031	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile