Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2033	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	22/06/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8255   GPS	Rainfall:	No Data
	Northing/Long.:	7647508 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	457550  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Pediment	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Eutrophic Brown Kandosol Medium Gravelly	Principal Profile Form:	Gn2.55
	 Clay-loamy Clay-loamy Deep
	ASC Confidence:	Great Soil Group:	No suitable group
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Hummock grass, 0.26-0.5m, Very sparse. *Species includes - Triodia pungens
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Melaleuca tamariscina
	Tall Strata - Tree mallee, 6.01-12m, Very sparse. *Species includes - Eucalyptus normantonensis, Eucalyptus similis
	Surface Coarse Fragments:	10-20%, medium gravelly, 6-20mm, subrounded, Sandstone
	Profile Morphology
	A1	0 - 0.07 m	Reddish brown (5YR4/4-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Dry;
	 Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.03); Clear change to 
	- 
	A12	0.07 - 0.24 m	Yellowish red (5YR4/6-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Dry; 
	Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.15); Clear change 
	to - 
	A2e	0.24 - 0.4 m	Yellowish brown (10YR5/4-Moist); ; Clayey sand (Heavy); Massive grade of structure; Earthy 
	fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.3); Clear
	 change to - 
	B2	0.4 - 1.5 m	Strong brown (7.5YR4/6-Moist); ; Clay loam, sandy; Earthy fabric; Dry; Very firm consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 1.2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2033	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2033	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile