Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2042	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	23/06/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8154   GPS	Rainfall:	No Data
	Northing/Long.:	7618270 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	437951  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Eutrophic Brown Chromosol Medium Non-gravelly Clay-	Principal Profile Form:	Db3.33
	loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Hummock grass, 0.51-1m, Mid-dense. *Species includes - TRIODIA SPECIES ?
	Mid Strata - Tree, 3.01-6m, Isolated plants. *Species includes - Melaleuca species
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus shirleyi, Eucalyptus normantonensis
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Brown (10YR4/3-Moist); ; Sandy clay loam (Light); Massive grade of structure; Earthy fabric; Dry; 
	Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Abrupt change to
	 - 
	A2j	0.1 - 0.25 m	Yellowish brown (10YR5/6-Moist); ; Clayey sand; Massive grade of structure; Earthy fabric; Dry; 
	Firm consistence; 0-2%, fine gravelly, 2-6mm, subrounded, Sandstone, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.2); Abrupt change to - 
	B21	0.25 - 0.3 m	Yellowish brown (10YR5/4-Moist); ; Clay loam, sandy; Weak grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Very strong consistence; 2-10%, fine gravelly, 2-
	6mm, subrounded, Sandstone, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.3); 
	2B21	0.3 - 0.4 m	Dark reddish brown (2.5YR3/4-Moist); ; Sandy light clay; Dry; 2-10%, fine gravelly, 2-6mm, 
	subrounded, Sandstone, coarse fragments; , Calcareous, , ; , Gypseous, , ; Soil matrix is 
	Slightly calcareous; 
	2B22	0.4 - 0.7 m	Pinkish grey (7.5YR7/3-Moist); ; Sandy light clay; Dry; , Calcareous, , ; , Gypseous, , ; Soil matrix
	 is Slightly calcareous; Field pH 9.5 (Raupach, 0.45); Field pH 8.5 (Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2042	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2042	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile