Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2043	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	23/06/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8154   GPS	Rainfall:	No Data
	Northing/Long.:	7618055 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	439680  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Kandosol Thin Non-gravelly Clay-loamy	Principal Profile Form:	Gn2.12
	 Clayey Deep
	ASC Confidence:	Great Soil Group:	Red earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - Aristida species, Eriachne species, TRIODIA SPECIES ?
	Mid Strata - , , . *Species includes - Hakea species, Petalostigma pubescens
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus shirleyi
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Dark yellowish brown (10YR3/4-Moist); ; Sandy clay loam; Massive grade of structure; Earthy 
	fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.04); Clear 
	change to - 
	B1	0.08 - 0.21 m	Strong brown (7.5YR4/6-Moist); ; Clay loam, sandy; Massive grade of structure, Polyhedral; 
	Earthy fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Firm consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.18); Clear change to - 
	B21	0.21 - 0.45 m	Strong brown (7.5YR4/6-Moist); Mottles, 2.5YR46, 10-20% , 0-5mm, Prominent; Mottles, 10-20% 
	; Clay loam, sandy; Weak grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; 
	Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Very firm consistence; 
	Common (10 - 20 %), Ferruginous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; 
	Field pH 6 (Raupach, 0.35); 
	B22	0.45 - 1.5 m	Yellowish red (5YR5/5-Moist); ; Sandy light clay; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 
	6.5 (Raupach, 1.2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2043	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2043	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile