Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2052	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	08/06/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8255   GPS	Rainfall:	No Data
	Northing/Long.:	7611886 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	477114  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting, Poached
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Hypocalcic Brown Dermosol Thin Non-gravelly Clayey 	Principal Profile Form:	Uf6.31
	Clayey Deep
	ASC Confidence:	Great Soil Group:	No suitable group
	No analytical data are available but confidence is fair.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Aristida species
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Acacia argyrodendron, Terminalia oblongata
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Acacia argyrodendron
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.09 m	Brown (10YR4/3-Moist); Mottles, 10YR46, 2-10% , 0-5mm, Prominent; Mottles, 2-10% ; Light 
	clay; Weak grade of structure, 5-10 mm, Platy; Rough-ped fabric; Dry; Very firm consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Gradual change to - 
	B21	0.09 - 0.35 m	Dark yellowish brown (10YR4/4-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ;
	 Field pH 6.5 (Raupach, 0.3); 
	B22	0.35 - 1.2 m	; Medium clay (Heavy); Dry; Strong consistence; 0-2%, fine gravelly, 2-6mm, subrounded, Quartz,
	 coarse fragments; , Calcareous, , ; , Gypseous, , ; Soil matrix is Moderately calcareous; Field 
	pH 8.5 (Raupach, 1.2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2052	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2052	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile