Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2060	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	09/06/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8255   GPS	Rainfall:	No Data
	Northing/Long.:	7609940 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	471362  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Self-Mulching Brown Vertosol Non-gravelly Medium 	Principal Profile Form:	Ug5.24
	fine Very fine Very deep 
	ASC Confidence:	Great Soil Group:	Brown clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Cenchrus ciliaris
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 1.01-3m, Very sparse. *Species includes - Acacia argyrodendron
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.08 m	Dark greyish brown (10YR4/2-Moist); ; Light clay; Moderate grade of structure, 2-5 mm, Granular; 
	Smooth-ped fabric; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 
	(Raupach, 0.04); Clear change to - 
	B1	0.08 - 0.25 m	Brown (10YR5/3-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Subangular 
	blocky; Smooth-ped fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 
	6.5 (Raupach, 0.15); Clear change to - 
	B21	0.25 - 0.6 m	Brown (10YR5/3-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 mm, 
	Subangular blocky; Weak grade of structure, Lenticular; Smooth-ped fabric; Dry; Strong 
	consistence; Few cutans, <10% of ped faces or walls coated, faint; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6 (Raupach, 0.4); Gradual change to - 
	B22	0.6 - 1.6 m	Pale brown (10YR6/3-Moist); ; Medium heavy clay; Strong grade of structure, 50-100 mm, 
	Subangular blocky; Moderate grade of structure, Lenticular; Smooth-ped fabric; Moderately 
	moist; Very firm consistence; 0-2%, fine gravelly, 2-6mm, subrounded, Sandstone, coarse 
	fragments; Common cutans, 10-50% of ped faces or walls coated, distinct; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6 (Raupach, 1.2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2060	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2060	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile