Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2083	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Bright, J (Mitch)	Locality:
	Date Desc.:	23/06/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8154   GPS	Rainfall:	No Data
	Northing/Long.:	7603656 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	442901  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Eutrophic Yellow Kandosol Thin Slightly gravelly Clay-	Principal Profile Form:	Gn4.82
	loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	Yellow earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Aristida species, Themeda triandra, Bothriochloa 
	decipiens	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Hakea species
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus melanophloia, Eucalyptus papuana
	Surface Coarse Fragments:	2-10%, coarse gravelly, 20-60mm, subrounded, Ironstone
	Profile Morphology
	A1	0 - 0.04 m	Very dark greyish brown (10YR3/2-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; 
	Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.03); Clear 
	change to - 
	A3	0.04 - 0.22 m	Dark brown (10YR3/3-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Dry; Weak 
	consistence; 0-2%, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 
	0.15); Gradual change to - 
	B1	0.22 - 0.55 m	Brownish yellow (10YR6/6-Moist); ; Light clay; Weak grade of structure, 5-10 mm, Polyhedral; 
	Rough-ped fabric; Dry; Firm consistence; 20-50%, fine gravelly, 2-6mm, rounded, dispersed, 
	Ironstone, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 0.4); 
	Diffuse change to - 
	B21	0.55 - 1.1 m	Brownish yellow (10YR6/6-Moist); Mottles, 2.5YR46, 0-2% , 0-5mm, Distinct; Mottles, 0-2% ; 
	Light clay; Weak grade of structure, 5-10 mm, Polyhedral; Rough-ped fabric; Dry; Very firm 
	consistence; 20-50%, fine gravelly, 2-6mm, rounded, dispersed, Ironstone, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 5 (Raupach, 0.8); Diffuse change to - 
	B22	1.1 - 1.3 m	Yellowish red (5YR4/6-Moist); ; Light clay; Weak grade of structure, 5-10 mm, Polyhedral; 
	Rough-ped fabric; Dry; Very firm consistence; 20-50%, fine gravelly, 2-6mm, rounded, dispersed,
	 Ironstone, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 1.2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2083	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2083	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile