Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2099	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	04/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7857   GPS	Rainfall:	No Data
	Northing/Long.:	7752140 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	286363  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Chromosol Thick Non-gravelly Loamy	Principal Profile Form:	Db1.22
	 Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Non-calcic brown 
	No analytical data are available but confidence is fair.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Bothriochloa decipiens
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus quadricostata, Eucalyptus polycarpa
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus quadricostata
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.03 m	Dark brown (7.5YR3/4-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; Weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.03); Clear change to - 
	A2	0.03 - 0.4 m	Dark yellowish brown (10YR4/4-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; 
	Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.15); Clear 
	change to - 
	B21	0.4 - 0.7 m	Strong brown (7.5YR4/6-Moist); ; Sandy light medium clay; Moderate grade of structure, 10-20 
	mm, Subangular blocky; Smooth-ped fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous,
	 , ; Field pH 7 (Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2099	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2099	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile