Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2101	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	04/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7857   GPS	Rainfall:	No Data
	Northing/Long.:	7752942 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	281444  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	10 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol Medium Slightly gravelly 	Principal Profile Form:	Dr2.12
	Clay-loamy Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	Non-calcic brown 
	Analytical data are incomplete but reasonable confidence.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Mid-dense. *Species includes - Bothriochloa ewartiana, Triodia mitchelii, 
	Themeda triandra	Mid Strata - Tree, 3.01-6m, Isolated plants. *Species includes - Eucalyptus crebra, Grevillea parallela, Eucalyptus 
	erythrophloia
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus crebra, Brachychiton populneus
	Surface Coarse Fragments:	2-10%, fine gravelly, 2-6mm, angular platy, Metamorphic rock (unidentified)
	Profile Morphology
	A	0 - 0.1 m	Brown (7.5YR4/4-Moist); ; Clay loam (Light); Massive grade of structure; Earthy fabric; Dry; Very 
	weak consistence; 2-10%, fine gravelly, 2-6mm, angular platy, dispersed, Metamorphic rock 
	(unidentified), coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); 
	B2	0.1 - 0.6 m	Dark red (2.5YR3/5-Moist); ; Light medium clay; Strong grade of structure, 5-10 mm, Angular 
	blocky; Smooth-ped fabric; Dry; Firm consistence; 10-20%, fine gravelly, 2-6mm, angular platy, 
	Metamorphic rock (unidentified), coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7 
	(Raupach, 0.4); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2101	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2101	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile