Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2110	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	05/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7857   GPS	Rainfall:	No Data
	Northing/Long.:	7773136 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	277674  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Closed Depression	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Self-Mulching Black Vertosol Medium Slightly gravelly 	Principal Profile Form:	Ug5.16
	Very fine Very deep 
	ASC Confidence:	Great Soil Group:	Black earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - None recorded
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - , , . *Species includes - None Recorded
	Surface Coarse Fragments:	2-10%, stony, 200-600mm, subrounded, Basalt
	Profile Morphology
	A11	0 - 0.15 m	Dark grey (2.5Y4/0-Moist); ; Light medium clay; Strong grade of structure, <2 mm, Granular; 
	Smooth-ped fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 
	(Raupach, 0.05); 
	A12	0.15 - 0.25 m	Very dark grey (2.5Y3/0-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Strong consistence; Common cutans, 10-50% of 
	ped faces or walls coated, distinct; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.2); 
	B21	0.25 - 0.75 m	Very dark grey (2.5Y3/0-Moist); ; Medium heavy clay; Strong grade of structure, 50-100 mm, 
	Lenticular; Strong grade of structure, 10-20 mm, Lenticular; Smooth-ped fabric; Moderately 
	moist; Strong consistence; Common cutans, 10-50% of ped faces or walls coated, distinct; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7.8 (Raupach, 0.6); 
	B22	0.75 - 1.1 m	Dark greenish grey (5GY4/1-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, 
	Lenticular; Strong grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; Moderately 
	moist; Strong consistence; Common cutans, 10-50% of ped faces or walls coated, distinct; , 
	Calcareous, , ; , Gypseous, , ; Field pH 8.5 (Raupach, 1); 
	B23	1.1 - 1.6 m	Olive grey (5Y5/2-Moist); ; Light medium clay; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; Moderately moist; Firm consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 8.5 (Raupach, 1.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2110	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2110	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile