Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2111	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	05/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7857   GPS	Rainfall:	No Data
	Northing/Long.:	7894055 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	270409  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Existing vertical exposure, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	Open depression (vale)	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Subnatric Grey Sodosol     	Principal Profile Form:	Dy2.43
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Isolated plants. *Species includes - Aristida species
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.18 m	Dark yellowish brown (10YR4/4-Moist); ; Sandy clay loam; Massive grade of structure; Earthy 
	fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 0.05); 
	A2e	0.18 - 0.33 m	Greyish brown (2.5Y5/2-Moist); ; Fine sandy loam (Heavy); Massive grade of structure; Earthy 
	fabric; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); 
	B21	0.33 - 0.5 m	Greyish brown (10YR5/2-Moist); Mottles, 2.5Y54, 2-10% , 0-5mm, Distinct; Mottles, 2-10% ; 
	Medium heavy clay; Strong grade of structure, 100-200 mm, Columnar; Strong grade of structure,
	 20-50 mm, Angular blocky; Smooth-ped fabric; Dry; Very strong consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7 (Raupach, 0.4); 
	B22	0.5 - 0.7 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium heavy clay; Strong grade of structure, 50-100 mm, 
	Angular blocky; Strong grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; Dry; 
	Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 8.5 (Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2111	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2111	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile