Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2113	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	06/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7858   GPS	Rainfall:	No Data
	Northing/Long.:	7789114 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	271544  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Mottled-Subnatric Grey Sodosol     	Principal Profile Form:	Dy2.43
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Aristida species
	Mid Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.02 m	Greyish brown (10YR5/2-Moist); ; Fine sandy clay loam; Massive grade of structure; Earthy 
	fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0); 
	A2e	0.02 - 0.12 m	Greyish brown (10YR5/2-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Dry;
	 Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.1); 
	B21	0.12 - 0.5 m	Greyish brown (10YR5/2-Moist); Mottles, 10YR58, 2-10% , 0-5mm, Distinct; Mottles, 2-10% ; 
	Medium heavy clay; Moderate grade of structure, 50-100 mm, Columnar; Smooth-ped fabric; Dry; 
	Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.4); 
	B22	0.5 - 0.6 m	Greyish brown (10YR5/2-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Smooth-ped fabric; Dry; Very strong consistence; , Calcareous, , ; , Gypseous, , 
	; Field pH 7 (Raupach, 0.6); 
	B23c	0.6 - 0.7 m	Pale brown (10YR6/3-Moist); ; Medium heavy clay; 20-50 mm, Angular blocky; Smooth-ped 
	fabric; Dry; Very strong consistence; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Nodules; , 
	Gypseous, , ; Field pH 9 (Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2113	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2113	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile