Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2117	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	06/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7858   GPS	Rainfall:	No Data
	Northing/Long.:	7796875 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	245539  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Manganic Mesotrophic Yellow Ferrosol Thin Non-gravelly 	Principal Profile Form:	Gn3.72
	Clay-loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Euchrozem
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Themeda triandra, Heteropogon contortus, 
	Bothriochloa species	Mid Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A	0 - 0.08 m	Very dark greyish brown (10YR3/2-Moist); ; Sandy clay loam; Weak grade of structure, 2-5 mm, 
	Columnar; Smooth-ped fabric; Dry; Few (2 - 10 %), , , ; , Calcareous, , ; , Gypseous, , ; Field pH 6
	 (Raupach, 0.05); 
	B11	0.08 - 0.28 m	Dark yellowish brown (10YR3/4-Moist); ; Clay loam; Moderate grade of structure, 5-10 mm, 
	Angular blocky; Smooth-ped fabric; Dry; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.2); 
	0.28 - 0.4 m	Brownish yellow (10YR6/8-Moist); ; Clay loam; Moderate grade of structure, 5-10 mm, Angular 
	blocky; Smooth-ped fabric; Many (20 - 50 %), Manganiferous, Coarse (6 - 20 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.4); 
	B2	0.4 - 0.8 m	Brownish yellow (10YR6/8-Moist); ; Light clay; Smooth-ped fabric; Dry; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.5 (Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2117	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2117	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile