Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2120	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	07/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7758   GPS	Rainfall:	No Data
	Northing/Long.:	7818125 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	232384  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Rises
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Mesotrophic Yellow Chromosol Thick Non-gravelly 	Principal Profile Form:	Dy3.32
	Sandy Clayey Deep
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	No analytical data are available but confidence is fair.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Bothriochloa species, Aristida species
	Mid Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.08 m	Dark greyish brown (10YR4/2-Moist); ; Coarse sand; Massive grade of structure; Earthy fabric; 
	Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); 
	A12	0.08 - 0.3 m	Brown (10YR5/3-Moist); ; Coarse sand; Massive grade of structure; Earthy fabric; Dry; Weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.25); 
	A2e	0.3 - 0.45 m	Yellowish brown (10YR5/4-Moist); ; Loamy coarse sand; Massive grade of structure; Earthy 
	fabric; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.4); 
	B1	0.45 - 0.6 m	Light yellowish brown (10YR6/4-Moist); ; Coarse sandy clay loam; Massive grade of structure; 
	Earthy fabric; Dry; Very strong consistence; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.5); 
	B21c	0.6 - 0.7 m	Grey (10YR6/1-Moist); Mottles, 10YR58, 10-20% , 5-15mm, Prominent; Mottles, 10-20% ; Medium
	 heavy clay; Moderate grade of structure, 10-20 mm, Subangular blocky; Earthy fabric; Dry; Very 
	strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.7); 
	B22	0.7 - 1.2 m	Dark yellowish brown (10YR4/6-Moist); ; Medium heavy clay; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2120	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2120	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile