Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2123	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	07/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7858   GPS	Rainfall:	No Data
	Northing/Long.:	7810700 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	241849  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Self-Mulching Grey Vertosol Slightly gravelly Fine Very 	Principal Profile Form:	Ug5.24
	fine Deep 
	ASC Confidence:	Great Soil Group:	Black earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Bothriochloa species
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - , , . *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.04 m	Grey (10YR5/1-Moist); ; Light clay; Strong grade of structure, 2-5 mm, Granular; Dry; Weak 
	consistence; 0-2%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; 
	Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; , Calcareous, , ; , Gypseous, , ; 
	Field pH 7.5 (Raupach, 0.02); 
	A12	0.04 - 0.2 m	Grey (10YR5/1-Moist); ; Medium heavy clay; Strong grade of structure, 50-100 mm, Angular 
	blocky; Dry; Strong consistence; 2-10%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, 
	coarse fragments; Common (10 - 20 %), Manganiferous, Fine (0 - 2 mm), Nodules; , Calcareous,
	 , ; , Gypseous, , ; Field pH 9.5 (Raupach, 0.15); 
	B21	0.2 - 1 m	Weak red (2.5YR4/1-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, 
	Lenticular; Moderately moist; Strong consistence; 2-10%, fine gravelly, 2-6mm, subrounded, 
	dispersed, Quartz, coarse fragments; Common cutans, 10-50% of ped faces or walls coated, 
	distinct; Common (10 - 20 %), Manganiferous, Fine (0 - 2 mm), Nodules; Few (2 - 10 %), 
	Calcareous, Fine (0 - 2 mm), Nodules; , Gypseous, , ; Field pH 9.5 (Raupach, 0.9); 
	B22	1 - 1.2 m	Weak red (2.5YR4/1-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, 
	Lenticular; Moderately moist; Strong consistence; 0-2%, fine gravelly, 2-6mm, subrounded, 
	dispersed, Quartz, coarse fragments; Common cutans, 10-50% of ped faces or walls coated, 
	distinct; Common (10 - 20 %), Manganiferous, Fine (0 - 2 mm), Nodules; Few (2 - 10 %), 
	Calcareous, Fine (0 - 2 mm), Nodules; , Gypseous, , ; Field pH 9.5 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2123	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2123	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile