Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2125	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	07/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7858   GPS	Rainfall:	No Data
	Northing/Long.:	7786714 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	278610  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Eutrophic Brown Chromosol     	Principal Profile Form:	Dy3.22
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	No analytical data are available but confidence is fair.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Isolated plants. *Species includes - None recorded
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus crebra
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.03 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy coarse sand; Massive grade of structure; 
	Earthy fabric; Dry; Weak consistence; 0-2%, fine gravelly, 2-6mm, subrounded, dispersed, 
	Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0); 
	A21	0.03 - 0.3 m	Dark greyish brown (10YR4/2-Moist); ; Loamy coarse sand (Heavy); Massive grade of structure; 
	Earthy fabric; Dry; Weak consistence; 0-2%, fine gravelly, 2-6mm, subrounded, dispersed, 
	Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.25); 
	0.3 - 0.5 m	Dark greyish brown (10YR4/2-Moist); ; Loamy sand; Massive grade of structure; Earthy fabric; 
	Weak consistence; 0-2%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse 
	fragments; Many (20 - 50 %), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.5 (Raupach, 0.4); 
	B21	0.5 - 1.2 m	Dark brown (7.5YR3/4-Moist); ; Sandy clay loam; Massive grade of structure; Smooth-ped fabric; 
	Dry; 0-2%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; , Calcareous,
	 , ; , Gypseous, , ; Field pH 7 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2125	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2125	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile