Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2136	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	19/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7959   GPS	Rainfall:	No Data
	Northing/Long.:	7883190 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	311057  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Sodic Eutrophic Brown Dermosol     	Principal Profile Form:	Gn3.35
	ASC Confidence:	Great Soil Group:	No suitable group
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Hummock grass, <0.25m, Isolated plants. *Species includes - Triodia mitchelii
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus persistens
	Surface Coarse Fragments:	20-50%, medium gravelly, 6-20mm, subangular platy, Ironstone
	Profile Morphology
	A11	0 - 0.08 m	Dark greyish brown (10YR4/2-Moist); ; Clay loam (Light); Massive grade of structure; Earthy 
	fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5 (Raupach, 0.05); 
	A2e	0.08 - 0.35 m	Yellowish brown (10YR5/4-Moist); , 7.5YR46; Fine sandy clay loam; Massive grade of structure; 
	Earthy fabric; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 
	0.3); 
	B21	0.35 - 0.5 m	Dark yellowish brown (10YR4/4-Moist); ; Coarse sandy light clay; Moderate grade of structure, 2-
	5 mm, Subangular blocky; Smooth-ped fabric; Dry; Very firm consistence; 2-10%, medium 
	gravelly, 6-20mm, subrounded, Quartz, coarse fragments; Few (2 - 10 %), Ferromanganiferous, 
	Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.5); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2136	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2136	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile