Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2140	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Bright, J (Mitch)	Locality:
	Date Desc.:	19/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7959   GPS	Rainfall:	No Data
	Northing/Long.:	7876629 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	309284  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Existing vertical exposure, Sandstone 
	Land Form
	Rel/Slope Class: 	Rolling rises 9-30m 10-32%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	12 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Red Chromosol     	Principal Profile Form:	Dr3.11
	ASC Confidence:	Great Soil Group:	No suitable group
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Hummock grass, 0.26-0.5m, Sparse. *Species includes - Triodia mitchelii, Themeda triandra
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Petalostigma pubescens
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus peltata
	Surface Coarse Fragments:	50-90%, coarse gravelly, 20-60mm, angular, Breccia
	Profile Morphology
	A1	0 - 0.15 m	Dark brown (7.5YR3/3-Moist); ; Sandy loam (Heavy); Massive grade of structure; Earthy fabric; 
	Dry; Firm consistence; 2-10%, medium gravelly, 6-20mm, angular tabular, Sandstone, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Gradual change to - 
	A2	0.15 - 0.3 m	Reddish brown (5YR4/4-Moist); ; Sandy clay loam; Weak grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Very firm consistence; 2-10%, medium gravelly, 6-
	20mm, angular tabular, Sandstone, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 
	6 (Raupach, 0.2); Clear change to - 
	B2	0.3 - 0.8 m	Red (2.5YR4/6-Moist); Mottles, 2.5YR44, 0-2% , 0-5mm, Prominent; Mottles, 0-2% ; Sandy light 
	medium clay; Moderate grade of structure, 10-20 mm, Subangular blocky; Strong grade of 
	structure, 5-10 mm, Angular blocky; Smooth-ped fabric; Dry; Strong consistence; 10-20%, 
	medium gravelly, 6-20mm, angular tabular, Sandstone, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6 (Raupach, 0.5); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2140	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2140	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile