Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2148	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	20/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7959   GPS	Rainfall:	No Data
	Northing/Long.:	7873720 AMG zone: 55	Runoff:	Very rapid
	Easting/Lat.:	302217  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Shale 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Subnatric Brown Sodosol     	Principal Profile Form:	Dy2.43
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Unknown species, Unknown species, Unknown 
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus persistens
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus persistens
	Surface Coarse Fragments:	2-10%, medium gravelly, 6-20mm, subangular, Jasper
	Profile Morphology
	A2e	0 - 0.2 m	Brown (7.5YR4/3-Moist); ; Fine sandy loam; Massive grade of structure; Earthy fabric; Dry; Firm 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Clear change to - 
	B1	0.2 - 0.31 m	Brown (7.5YR5/3-Moist); ; Light medium clay; Moderate grade of structure, 5-10 mm, Subangular
	 blocky; Smooth-ped fabric; Dry; Very strong consistence; 10-20%, coarse gravelly, 20-60mm, 
	subangular, Ironstone, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 
	(Raupach, 0.25); Clear change to - 
	B21	0.31 - 0.55 m	Yellowish brown (10YR5/4-Moist); ; Light medium clay; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Very strong consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 8 (Raupach, 0.4); Gradual change to - 
	C	0.55 - 0.65 m	; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 9 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2148	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2148	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile